; Installation INF for the Cypress Generic USB Driver for Windows 2000
; Processor support for x86 based platforms.
;
; (c) Copyright 2011 Cypress Semiconductor Corporation
;

[Version]
Signature="$WINDOWS NT$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%CYUSB_Provider%
CatalogFile=CYUSB.cat
DriverVer=10/17/2011,3.4.7.000

[SourceDisksNames]
1=%CYUSB_Install%,,,

[SourceDisksFiles]
CYUSB.sys = 1

[DestinationDirs]
CYUSB.Files.Ext = 10,System32\Drivers

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%CYUSB_Provider%=Device,NT,NTx86,NTamd64

;for all platforms
[Device]
;%VID_XXXX&PID_XXXX.DeviceDesc%=CyUsb, USB\VID_XXXX&PID_XXXX
; Cypress FX2LP default ID
%VID_AAB4&PID_8613.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_8613
%VID_AAB4&PID_6473.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_AAB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_1004
%VID_ABB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ABB4&PID_1004
;150
%VID_ACB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ACB4&PID_1004
%VID_04B4&PID_8613.DeviceDesc%=CyUsb, USB\VID_04B4&PID_8613
%VID_04B4&PID_6473.DeviceDesc%=CyUsb, USB\VID_04B4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_04B4&PID_1004.DeviceDesc%=CyUsb, USB\VID_04B4&PID_1004
%VID_ACFF&PID_9999.DeviceDesc%=CyUsb, USB\VID_ACFF&PID_9999
%VID_AA25&PID_4210.DeviceDesc%=CyUsb, USB\VID_AA25&PID_4210
%VID_AA55&PID_2501.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2501
%VID_AA55&PID_2502.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2502
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
%VID_B300&PID_3601.DeviceDesc%=CyUsb, USB\VID_B300&PID_3601
%VID_B300&PID_3602.DeviceDesc%=CyUsb, USB\VID_B300&PID_3602
%VID_B310&PID_3602.DeviceDesc%=CyUsb, USB\VID_B310&PID_3602
%VID_B310&PID_3601.DeviceDesc%=CyUsb, USB\VID_B310&PID_3601

%VID_B330&PID_3202.DeviceDesc%=CyUsb, USB\VID_B330&PID_3202

%VID_A710&PID_3601.DeviceDesc%=CyUsb, USB\VID_A710&PID_3601
%VID_A710&PID_3602.DeviceDesc%=CyUsb, USB\VID_A710&PID_3602
%VID_A800&PID_3602.DeviceDesc%=CyUsb, USB\VID_A800&PID_3602
%VID_A800&PID_3601.DeviceDesc%=CyUsb, USB\VID_A800&PID_3601

%VID_A290&PID_3601.DeviceDesc%=CyUsb, USB\VID_A290&PID_3601
%VID_A290&PID_3602.DeviceDesc%=CyUsb, USB\VID_A290&PID_3602
%VID_F290&PID_3602.DeviceDesc%=CyUsb, USB\VID_F290&PID_3602
%VID_F290&PID_3601.DeviceDesc%=CyUsb, USB\VID_F290&PID_3601

%VID_AA55&PID_3601.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3601
%VID_AA55&PID_3602.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3602

%VID_B550&PID_3601.DeviceDesc%=CyUsb, USB\VID_B550&PID_3601
%VID_B550&PID_3602.DeviceDesc%=CyUsb, USB\VID_B550&PID_3602

%VID_A567&PID_3602.DeviceDesc%=CyUsb, USB\VID_A567&PID_3602
%VID_A678&PID_2541.DeviceDesc%=CyUsb, USB\VID_A678&PID_2541
%VID_5789&PID_E098.DeviceDesc%=CyUsb, USB\VID_5789&PID_E098
%VID_5789&PID_E795.DeviceDesc%=CyUsb, USB\VID_5789&PID_E795
%VID_5789&PID_3200.DeviceDesc%=CyUsb, USB\VID_5789&PID_3200
;VID_5789&PID_E098.DeviceDesc="BJ-USB Inkjet -5789e098  FV5.00(3.4.7.000 For WIN7 32Bit)"
;VID_5789&PID_38A3.DeviceDesc="UV ColorInkJet FV3.20(3.4.7.000 For WIN7 64Bit)"
%VID_5789&PID_38A3.DeviceDesc%=CyUsb, USB\VID_5789&PID_38A3
;for windows 2000 non intel platforms
[Device.NT]
;%VID_XXXX&PID_XXXX.DeviceDesc%=CyUsb, USB\VID_XXXX&PID_XXXX
; Cypress FX2LP default ID
%VID_AAB4&PID_8613.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_8613
%VID_AAB4&PID_6473.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_AAB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_1004
%VID_ABB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ABB4&PID_1004
;150
%VID_ACB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ACB4&PID_1004
%VID_04B4&PID_8613.DeviceDesc%=CyUsb, USB\VID_04B4&PID_8613
%VID_04B4&PID_6473.DeviceDesc%=CyUsb, USB\VID_04B4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_04B4&PID_1004.DeviceDesc%=CyUsb, USB\VID_04B4&PID_1004
%VID_ACFF&PID_9999.DeviceDesc%=CyUsb, USB\VID_ACFF&PID_9999
%VID_AA25&PID_4210.DeviceDesc%=CyUsb, USB\VID_AA25&PID_4210
%VID_AA55&PID_2501.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2501
%VID_AA55&PID_2502.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2502
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
%VID_B300&PID_3601.DeviceDesc%=CyUsb, USB\VID_B300&PID_3601
%VID_B300&PID_3602.DeviceDesc%=CyUsb, USB\VID_B300&PID_3602
%VID_B310&PID_3602.DeviceDesc%=CyUsb, USB\VID_B310&PID_3602
%VID_B310&PID_3601.DeviceDesc%=CyUsb, USB\VID_B310&PID_3601

%VID_B330&PID_3202.DeviceDesc%=CyUsb, USB\VID_B330&PID_3202

%VID_A710&PID_3601.DeviceDesc%=CyUsb, USB\VID_A710&PID_3601
%VID_A710&PID_3602.DeviceDesc%=CyUsb, USB\VID_A710&PID_3602
%VID_A800&PID_3602.DeviceDesc%=CyUsb, USB\VID_A800&PID_3602
%VID_A800&PID_3601.DeviceDesc%=CyUsb, USB\VID_A800&PID_3601

%VID_A290&PID_3601.DeviceDesc%=CyUsb, USB\VID_A290&PID_3601
%VID_A290&PID_3602.DeviceDesc%=CyUsb, USB\VID_A290&PID_3602
%VID_F290&PID_3602.DeviceDesc%=CyUsb, USB\VID_F290&PID_3602
%VID_F290&PID_3601.DeviceDesc%=CyUsb, USB\VID_F290&PID_3601

%VID_AA55&PID_3601.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3601
%VID_AA55&PID_3602.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3602

%VID_B550&PID_3601.DeviceDesc%=CyUsb, USB\VID_B550&PID_3601
%VID_B550&PID_3602.DeviceDesc%=CyUsb, USB\VID_B550&PID_3602
%VID_A567&PID_3602.DeviceDesc%=CyUsb, USB\VID_A567&PID_3602
%VID_A678&PID_2541.DeviceDesc%=CyUsb, USB\VID_A678&PID_2541
%VID_5789&PID_E098.DeviceDesc%=CyUsb, USB\VID_5789&PID_E098
%VID_5789&PID_E795.DeviceDesc%=CyUsb, USB\VID_5789&PID_E795
%VID_5789&PID_3200.DeviceDesc%=CyUsb, USB\VID_5789&PID_3200
;VID_5789&PID_E098.DeviceDesc="BJ-USB Inkjet -5789e098  FV5.00(3.4.7.000 For WIN7 32Bit)"
;VID_5789&PID_38A3.DeviceDesc="UV ColorInkJet FV3.20(3.4.7.000 For WIN7 64Bit)"
%VID_5789&PID_38A3.DeviceDesc%=CyUsb, USB\VID_5789&PID_38A3
;for x86 platforms
[Device.NTx86]
;%VID_XXXX&PID_XXXX.DeviceDesc%=CyUsb, USB\VID_XXXX&PID_XXXX
; Cypress FX2LP default ID
%VID_AAB4&PID_8613.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_8613
%VID_AAB4&PID_6473.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_AAB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_1004
%VID_ABB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ABB4&PID_1004
;150
%VID_ACB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ACB4&PID_1004
%VID_04B4&PID_8613.DeviceDesc%=CyUsb, USB\VID_04B4&PID_8613
%VID_04B4&PID_6473.DeviceDesc%=CyUsb, USB\VID_04B4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_04B4&PID_1004.DeviceDesc%=CyUsb, USB\VID_04B4&PID_1004
%VID_ACFF&PID_9999.DeviceDesc%=CyUsb, USB\VID_ACFF&PID_9999
%VID_AA25&PID_4210.DeviceDesc%=CyUsb, USB\VID_AA25&PID_4210
%VID_AA55&PID_2501.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2501
%VID_AA55&PID_2502.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2502
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
%VID_B300&PID_3601.DeviceDesc%=CyUsb, USB\VID_B300&PID_3601
%VID_B300&PID_3602.DeviceDesc%=CyUsb, USB\VID_B300&PID_3602
%VID_B310&PID_3602.DeviceDesc%=CyUsb, USB\VID_B310&PID_3602
%VID_B310&PID_3601.DeviceDesc%=CyUsb, USB\VID_B310&PID_3601

%VID_B330&PID_3202.DeviceDesc%=CyUsb, USB\VID_B330&PID_3202

%VID_A710&PID_3601.DeviceDesc%=CyUsb, USB\VID_A710&PID_3601
%VID_A710&PID_3602.DeviceDesc%=CyUsb, USB\VID_A710&PID_3602
%VID_A800&PID_3602.DeviceDesc%=CyUsb, USB\VID_A800&PID_3602
%VID_A800&PID_3601.DeviceDesc%=CyUsb, USB\VID_A800&PID_3601

%VID_A290&PID_3601.DeviceDesc%=CyUsb, USB\VID_A290&PID_3601
%VID_A290&PID_3602.DeviceDesc%=CyUsb, USB\VID_A290&PID_3602
%VID_F290&PID_3602.DeviceDesc%=CyUsb, USB\VID_F290&PID_3602
%VID_F290&PID_3601.DeviceDesc%=CyUsb, USB\VID_F290&PID_3601

%VID_AA55&PID_3601.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3601
%VID_AA55&PID_3602.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3602

%VID_B550&PID_3601.DeviceDesc%=CyUsb, USB\VID_B550&PID_3601
%VID_B550&PID_3602.DeviceDesc%=CyUsb, USB\VID_B550&PID_3602
%VID_A567&PID_3602.DeviceDesc%=CyUsb, USB\VID_A567&PID_3602
%VID_A678&PID_2541.DeviceDesc%=CyUsb, USB\VID_A678&PID_2541
%VID_5789&PID_E098.DeviceDesc%=CyUsb, USB\VID_5789&PID_E098
%VID_5789&PID_E795.DeviceDesc%=CyUsb, USB\VID_5789&PID_E795
%VID_5789&PID_3200.DeviceDesc%=CyUsb, USB\VID_5789&PID_3200
;VID_5789&PID_E098.DeviceDesc="BJ-USB Inkjet -5789e098  FV5.00(3.4.7.000 For WIN7 32Bit)"
;VID_5789&PID_38A3.DeviceDesc="UV ColorInkJet FV3.20(3.4.7.000 For WIN7 64Bit)"
%VID_5789&PID_38A3.DeviceDesc%=CyUsb, USB\VID_5789&PID_38A3
;for x64 platforms
[Device.NTamd64]
;%VID_XXXX&PID_XXXX.DeviceDesc%=CyUsb, USB\VID_XXXX&PID_XXXX
; Cypress FX2LP default ID
%VID_AAB4&PID_8613.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_8613
%VID_AAB4&PID_6473.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_AAB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_AAB4&PID_1004
%VID_ABB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ABB4&PID_1004
;150
%VID_ACB4&PID_1004.DeviceDesc%=CyUsb, USB\VID_ACB4&PID_1004
%VID_04B4&PID_8613.DeviceDesc%=CyUsb, USB\VID_04B4&PID_8613
%VID_04B4&PID_6473.DeviceDesc%=CyUsb, USB\VID_04B4&PID_6473
; Cypress FX2LP Example Device.  DVK firmware examples use this VID/PID
%VID_04B4&PID_1004.DeviceDesc%=CyUsb, USB\VID_04B4&PID_1004
%VID_ACFF&PID_9999.DeviceDesc%=CyUsb, USB\VID_ACFF&PID_9999
%VID_AA25&PID_4210.DeviceDesc%=CyUsb, USB\VID_AA25&PID_4210
%VID_AA55&PID_2501.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2501
%VID_AA55&PID_2502.DeviceDesc%=CyUsb, USB\VID_AA55&PID_2502
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
%VID_B300&PID_3601.DeviceDesc%=CyUsb, USB\VID_B300&PID_3601
%VID_B300&PID_3602.DeviceDesc%=CyUsb, USB\VID_B300&PID_3602
%VID_B310&PID_3602.DeviceDesc%=CyUsb, USB\VID_B310&PID_3602
%VID_B310&PID_3601.DeviceDesc%=CyUsb, USB\VID_B310&PID_3601

%VID_B330&PID_3202.DeviceDesc%=CyUsb, USB\VID_B330&PID_3202

%VID_A710&PID_3601.DeviceDesc%=CyUsb, USB\VID_A710&PID_3601
%VID_A710&PID_3602.DeviceDesc%=CyUsb, USB\VID_A710&PID_3602
%VID_A800&PID_3602.DeviceDesc%=CyUsb, USB\VID_A800&PID_3602
%VID_A800&PID_3601.DeviceDesc%=CyUsb, USB\VID_A800&PID_3601

%VID_A290&PID_3601.DeviceDesc%=CyUsb, USB\VID_A290&PID_3601
%VID_A290&PID_3602.DeviceDesc%=CyUsb, USB\VID_A290&PID_3602
%VID_F290&PID_3602.DeviceDesc%=CyUsb, USB\VID_F290&PID_3602
%VID_F290&PID_3601.DeviceDesc%=CyUsb, USB\VID_F290&PID_3601

%VID_AA55&PID_3601.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3601
%VID_AA55&PID_3602.DeviceDesc%=CyUsb, USB\VID_AA55&PID_3602

%VID_B550&PID_3601.DeviceDesc%=CyUsb, USB\VID_B550&PID_3601
%VID_B550&PID_3602.DeviceDesc%=CyUsb, USB\VID_B550&PID_3602
%VID_A567&PID_3602.DeviceDesc%=CyUsb, USB\VID_A567&PID_3602
%VID_A678&PID_2541.DeviceDesc%=CyUsb, USB\VID_A678&PID_2541
%VID_5789&PID_E098.DeviceDesc%=CyUsb, USB\VID_5789&PID_E098
%VID_5789&PID_E795.DeviceDesc%=CyUsb, USB\VID_5789&PID_E795
%VID_5789&PID_3200.DeviceDesc%=CyUsb, USB\VID_5789&PID_3200
;VID_5789&PID_E098.DeviceDesc="BJ-USB Inkjet -5789e098  FV5.00(3.4.7.000 For WIN7 32Bit)"
;VID_5789&PID_38A3.DeviceDesc="UV ColorInkJet FV3.20(3.4.7.000 For WIN7 64Bit)"
%VID_5789&PID_38A3.DeviceDesc%=CyUsb, USB\VID_5789&PID_38A3
[CYUSB]
CopyFiles=CYUSB.Files.Ext
AddReg=CyUsb.AddReg

[CYUSB.HW]
AddReg=CYUSB.AddReg.Guid

[CYUSB.Services]
Addservice = CYUSB,2,CYUSB.AddService

[CYUSB.NT]
CopyFiles=CYUSB.Files.Ext
AddReg=CyUsb.AddReg

[CYUSB.NT.HW]
AddReg=CYUSB.AddReg.Guid

[CYUSB.NT.Services]
Addservice = CYUSB,2,CYUSB.AddService


[CYUSB.NTx86]
CopyFiles=CYUSB.Files.Ext
AddReg=CyUsb.AddReg

[CYUSB.NTx86.HW]
AddReg=CYUSB.AddReg.Guid

[CYUSB.NTx86.Services]
Addservice = CYUSB,2,CYUSB.AddService

[CYUSB.NTamd64]
CopyFiles=CYUSB.Files.Ext
AddReg=CyUsb.AddReg

[CYUSB.NTamd64.HW]
AddReg=CYUSB.AddReg.Guid

[CYUSB.NTamd64.Services]
Addservice = CYUSB,2,CYUSB.AddService


[CYUSB.AddReg]
; Deprecating - do not use in new apps to identify a CYUSB driver
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,CYUSB.sys
; You may optionally include a check for DriverBase in your application to check for a CYUSB driver
HKR,,DriverBase,,CYUSB.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR,,FriendlyName,,%CYUSB_Description%

[CYUSB.AddService]
DisplayName    = %CYUSB_Description%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\CYUSB.sys
AddReg         = CYUSB.AddReg
LoadOrderGroup = Base

[CYUSB.Files.Ext]
CYUSB.sys

[CYUSB.AddReg.Guid]
HKR,,DriverGUID,,%CYUSB.GUID%

[Strings]
CYUSB_Provider    = "Cypress"
CYUSB_Company     = "Cypress Semiconductor Corporation"
CYUSB_Description = "Cypress Generic USB Driver"
CYUSB_DisplayName = "Cypress USB Generic"
CYUSB_Install     = "Cypress CYUSB Driver Installation Disk"
VID_XXXX&PID_XXXX.DeviceDesc="Cypress USB Generic Driver (3.4.7.000)"
VID_04B4&PID_8613.DeviceDesc="BJ2502 Printer - ep missing(3.4.7.000 For XP32Bit)"
VID_04B4&PID_6473.DeviceDesc="BJ - EEPROM missing(3.4.7.000 For XP64Bit)"
VID_AAB4&PID_8613.DeviceDesc="BJ-USB Inkjet -BJ2541 - ep missing(3.4.7.000 For WIN2000-32Bit)"
VID_ACB4&PID_1004.DeviceDesc="BJ-USB Inkjet -BJ2542  FV1.00(3.4.7.000 For WIN2000-32Bit)"
;VID_ACB4&PID_2544.DeviceDesc="BJ-USB Inkjet -BJ2544  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_AA55&PID_2501.DeviceDesc="BJ-USB Inkjet -BJ2501  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_AA55&PID_2502.DeviceDesc="BJ-USB Inkjet -BJ2502  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_ACFF&PID_9999.DeviceDesc="BJ-USB Inkjet -FireDriver dog(3.4.7.000 For WIN2000-32Bit)"
VID_AA25&PID_4210.DeviceDesc="BJ-USB Inkjet -BJ2542 Firmware1.0(3.4.7.000 For WIN2000-32Bit)"
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
VID_B300&PID_3601.DeviceDesc="BJ-USB Inkjet -B300-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_B300&PID_3602.DeviceDesc="BJ-USB Inkjet -B300-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_AA55&PID_3601.DeviceDesc="BJ-USB Inkjet -R800-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_AA55&PID_3602.DeviceDesc="BJ-USB Inkjet -R800-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_B310&PID_3601.DeviceDesc="BJ-USB Inkjet -B310-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_B310&PID_3602.DeviceDesc="BJ-USB Inkjet -B310-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"

VID_B330&PID_3202.DeviceDesc="BJ-USB Inkjet -B330-3202  FV3.00(3.4.7.000 For WIN2000-32Bit)"

VID_A710&PID_3601.DeviceDesc="BJ-USB Inkjet -A710-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_A710&PID_3602.DeviceDesc="BJ-USB Inkjet -A710-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_A567&PID_3602.DeviceDesc="BJ-USB Inkjet -A567-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_A678&PID_2541.DeviceDesc="BJ-USB Inkjet -A678-2541  FV1.00(3.4.7.000 For WIN2000-32Bit)"
;

VID_A800&PID_3601.DeviceDesc="BJ-USB Inkjet -A800-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_A800&PID_3602.DeviceDesc="BJ-USB Inkjet -A800-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"

VID_A290&PID_3601.DeviceDesc="BJ-USB Inkjet -A290-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_A290&PID_3602.DeviceDesc="BJ-USB Inkjet -A290-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"

VID_F290&PID_3601.DeviceDesc="BJ-USB Inkjet -F290-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_F290&PID_3602.DeviceDesc="BJ-USB Inkjet -F290-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"

VID_B550&PID_3601.DeviceDesc="BJ-USB Inkjet -B550-3601  FV1.00(3.4.7.000 For WIN2000-32Bit)"
VID_B550&PID_3602.DeviceDesc="BJ-USB Inkjet -B550-3602  FV1.00(3.4.7.000 For WIN2000-32Bit)"
;%VID_5789&PID_E098.DeviceDesc%=CyUsb, USB\VID_5789&PID_E098
VID_5789&PID_E098.DeviceDesc="BJ-USB Inkjet -5789e098  FV5.00(3.4.7.000 For WIN7 32Bit)"
VID_5789&PID_E795.DeviceDesc="YICAI  FV5.00(3.4.7.000 For WIN7 64Bit/32bit)"
VID_5789&PID_3200.DeviceDesc="UV-ColorInkJetPrinter  FV3.20(3.4.7.000 For WIN7 64Bit/32bit)"
VID_5789&PID_38A3.DeviceDesc="UV ColorInkJet FV3.20(3.4.7.000 For WIN7 64Bit)"
;%VID_5789&PID_38A3.DeviceDesc%=CyUsb, USB\VID_5789&PID_38A3
CYUSB.GUID="{AE18AA60-7F6A-11d4-97DD-00010229B959}"
CYUSB_Unused      = "."
